(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")

  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 145)
    (zones 0)
    (modules 4)
    (nets 45)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J3-Pad1)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(J3-Pad3)")
  (net 8 "Net-(J3-Pad4)")
  (net 9 "Net-(J3-Pad5)")
  (net 10 "Net-(J3-Pad6)")
  (net 11 "Net-(J3-Pad7)")
  (net 12 "Net-(J3-Pad8)")
  (net 13 "Net-(J3-Pad9)")
  (net 14 "Net-(J3-Pad10)")
  (net 15 "Net-(J3-Pad11)")
  (net 16 "Net-(J3-Pad12)")
  (net 17 "Net-(J3-Pad13)")
  (net 18 "Net-(J3-Pad14)")
  (net 19 "Net-(J3-Pad15)")
  (net 20 "Net-(J3-Pad16)")
  (net 21 "Net-(J3-Pad17)")
  (net 22 "Net-(J3-Pad18)")
  (net 23 "Net-(J3-Pad19)")
  (net 24 "Net-(J3-Pad20)")
  (net 25 "Net-(J3-Pad21)")
  (net 26 "Net-(J3-Pad22)")
  (net 27 "Net-(J3-Pad23)")
  (net 28 "Net-(J3-Pad24)")
  (net 29 "Net-(J3-Pad25)")
  (net 30 "Net-(J3-Pad26)")
  (net 31 "Net-(J3-Pad27)")
  (net 32 "Net-(J3-Pad28)")
  (net 33 "Net-(J3-Pad29)")
  (net 34 "Net-(J3-Pad30)")
  (net 35 "Net-(J3-Pad31)")
  (net 36 "Net-(J3-Pad32)")
  (net 37 "Net-(J3-Pad33)")
  (net 38 "Net-(J3-Pad34)")
  (net 39 "Net-(J3-Pad35)")
  (net 40 "Net-(J3-Pad36)")
  (net 41 "Net-(J3-Pad37)")
  (net 42 "Net-(J3-Pad38)")
  (net 43 "Net-(J3-Pad39)")
  (net 44 "Net-(J3-Pad40)")

  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad14)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad18)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad20)")
    (add_net "Net-(J3-Pad21)")
    (add_net "Net-(J3-Pad22)")
    (add_net "Net-(J3-Pad23)")
    (add_net "Net-(J3-Pad24)")
    (add_net "Net-(J3-Pad25)")
    (add_net "Net-(J3-Pad26)")
    (add_net "Net-(J3-Pad27)")
    (add_net "Net-(J3-Pad28)")
    (add_net "Net-(J3-Pad29)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad30)")
    (add_net "Net-(J3-Pad31)")
    (add_net "Net-(J3-Pad32)")
    (add_net "Net-(J3-Pad33)")
    (add_net "Net-(J3-Pad34)")
    (add_net "Net-(J3-Pad35)")
    (add_net "Net-(J3-Pad36)")
    (add_net "Net-(J3-Pad37)")
    (add_net "Net-(J3-Pad38)")
    (add_net "Net-(J3-Pad39)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad40)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
  )

  (module Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal (layer F.Cu) (tedit 5AEE14E3) (tstamp 6031EC2B)
    (at 43.85 50.4 270)
    (descr "TE FPC connector, 04 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4")
    (tags "te fpc 84952")
    (path /606FA278)
    (attr smd)
    (fp_text reference J2 (at 0 -4 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 7.7 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.46 -3.3) (end -6.46 -3.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.46 7) (end 6.46 -3.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.46 7) (end 6.46 7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.46 -3.3) (end -6.46 7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.065 -0.91) (end 2.89 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.065 -0.91) (end -2.065 -2.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.89 -0.91) (end -2.065 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.045 3.6) (end -5.045 3.06) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.07 3.6) (end -5.045 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.07 4.71) (end -6.07 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.07 4.71) (end -6.07 4.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.07 3.6) (end 6.07 4.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.045 3.6) (end 6.07 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.045 3.06) (end 5.045 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.935 5.61) (end -4.935 4.6) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 5.61) (end -4.935 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 6.5) (end -5.96 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 6.5) (end -5.96 6.5) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 5.61) (end 5.96 6.5) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 5.61) (end 5.96 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 4.6) (end 4.935 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 0.2) (end -1 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -0.8) (end -1.5 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -4.935 3.71) (end -4.935 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 3.71) (end -4.935 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 4.6) (end -5.96 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 4.6) (end -5.96 4.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 3.71) (end 5.96 4.6) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 3.71) (end 5.96 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 -0.8) (end 4.935 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start -4.935 -0.8) (end 4.935 -0.8) (layer F.Fab) (width 0.1))
    (pad MP smd rect (at 4.49 1 270) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at -4.49 1 270) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at 0.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -0.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -1.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_84952-4_1x04-1MP_P1.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal (layer F.Cu) (tedit 5AEE14E3) (tstamp 6031FA80)
    (at 44.89 39.6 180)
    (descr "TE FPC connector, 04 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4")
    (tags "te fpc 84952")
    (path /606F93E2)
    (attr smd)
    (fp_text reference J1 (at 0 -4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 7.7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.46 -3.3) (end -6.46 -3.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.46 7) (end 6.46 -3.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.46 7) (end 6.46 7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.46 -3.3) (end -6.46 7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.065 -0.91) (end 2.89 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.065 -0.91) (end -2.065 -2.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.89 -0.91) (end -2.065 -0.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.045 3.6) (end -5.045 3.06) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.07 3.6) (end -5.045 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.07 4.71) (end -6.07 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.07 4.71) (end -6.07 4.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.07 3.6) (end 6.07 4.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.045 3.6) (end 6.07 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.045 3.06) (end 5.045 3.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.935 5.61) (end -4.935 4.6) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 5.61) (end -4.935 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 6.5) (end -5.96 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 6.5) (end -5.96 6.5) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 5.61) (end 5.96 6.5) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 5.61) (end 5.96 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 4.6) (end 4.935 5.61) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 0.2) (end -1 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -0.8) (end -1.5 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -4.935 3.71) (end -4.935 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 3.71) (end -4.935 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start -5.96 4.6) (end -5.96 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 4.6) (end -5.96 4.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5.96 3.71) (end 5.96 4.6) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 3.71) (end 5.96 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start 4.935 -0.8) (end 4.935 3.71) (layer F.Fab) (width 0.1))
    (fp_line (start -4.935 -0.8) (end 4.935 -0.8) (layer F.Fab) (width 0.1))
    (pad MP smd rect (at 4.49 1 180) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at -4.49 1 180) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_84952-4_1x04-1MP_P1.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_FFC-FPC:Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal (layer F.Cu) (tedit 5D24667B) (tstamp 6031F0A1)
    (at 64.9 39.3 180)
    (descr "Hirose FH12, FFC/FPC connector, FH12-40S-0.5SH, 40 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (path /606FBFA7)
    (attr smd)
    (fp_text reference J3 (at 0 -3.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x40 (at 0 5.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -1.2) (end -11.55 -1.2) (layer F.Fab) (width 0.1))
    (fp_line (start -11.55 -1.2) (end -11.55 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -11.55 3.4) (end -10.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -10.95 3.4) (end -10.95 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start -10.95 3.7) (end -11.45 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start -11.45 3.7) (end -11.45 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start -11.45 4.4) (end 0 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -1.2) (end 11.55 -1.2) (layer F.Fab) (width 0.1))
    (fp_line (start 11.55 -1.2) (end 11.55 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 11.55 3.4) (end 10.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 10.95 3.4) (end 10.95 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start 10.95 3.7) (end 11.45 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start 11.45 3.7) (end 11.45 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start 11.45 4.4) (end 0 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start -10.16 -1.3) (end -11.65 -1.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.65 -1.3) (end -11.65 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 -1.3) (end 11.65 -1.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.65 -1.3) (end 11.65 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.65 2.76) (end -11.65 4.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.65 4.5) (end 11.65 4.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.65 4.5) (end 11.65 2.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.16 -1.3) (end -10.16 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.25 -1.2) (end -9.75 -0.492893) (layer F.Fab) (width 0.1))
    (fp_line (start -9.75 -0.492893) (end -9.25 -1.2) (layer F.Fab) (width 0.1))
    (fp_line (start -13.05 -3) (end -13.05 4.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -13.05 4.9) (end 13.05 4.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.05 4.9) (end 13.05 -3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.05 -3) (end -13.05 -3) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 3.7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad MP smd rect (at 11.65 1.4 180) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at -11.65 1.4 180) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -9.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -9.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at -8.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at -8.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at -7.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad5)"))
    (pad 6 smd rect (at -7.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad6)"))
    (pad 7 smd rect (at -6.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad7)"))
    (pad 8 smd rect (at -6.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad8)"))
    (pad 9 smd rect (at -5.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J3-Pad9)"))
    (pad 10 smd rect (at -5.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J3-Pad10)"))
    (pad 11 smd rect (at -4.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad11)"))
    (pad 12 smd rect (at -4.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad12)"))
    (pad 13 smd rect (at -3.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad13)"))
    (pad 14 smd rect (at -3.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad14)"))
    (pad 15 smd rect (at -2.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-Pad15)"))
    (pad 16 smd rect (at -2.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad16)"))
    (pad 17 smd rect (at -1.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad17)"))
    (pad 18 smd rect (at -1.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad18)"))
    (pad 19 smd rect (at -0.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad19)"))
    (pad 20 smd rect (at -0.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad20)"))
    (pad 21 smd rect (at 0.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad21)"))
    (pad 22 smd rect (at 0.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad22)"))
    (pad 23 smd rect (at 1.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J3-Pad23)"))
    (pad 24 smd rect (at 1.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-Pad24)"))
    (pad 25 smd rect (at 2.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J3-Pad25)"))
    (pad 26 smd rect (at 2.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J3-Pad26)"))
    (pad 27 smd rect (at 3.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J3-Pad27)"))
    (pad 28 smd rect (at 3.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J3-Pad28)"))
    (pad 29 smd rect (at 4.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J3-Pad29)"))
    (pad 30 smd rect (at 4.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J3-Pad30)"))
    (pad 31 smd rect (at 5.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J3-Pad31)"))
    (pad 32 smd rect (at 5.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J3-Pad32)"))
    (pad 33 smd rect (at 6.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J3-Pad33)"))
    (pad 34 smd rect (at 6.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J3-Pad34)"))
    (pad 35 smd rect (at 7.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J3-Pad35)"))
    (pad 36 smd rect (at 7.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad36)"))
    (pad 37 smd rect (at 8.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J3-Pad37)"))
    (pad 38 smd rect (at 8.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J3-Pad38)"))
    (pad 39 smd rect (at 9.25 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J3-Pad39)"))
    (pad 40 smd rect (at 9.75 -1.85 180) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J3-Pad40)"))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_FFC-FPC:Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal (layer F.Cu) (tedit 5D24667B) (tstamp 6031ECC1)
    (at 64.875 51.875)
    (descr "Hirose FH12, FFC/FPC connector, FH12-40S-0.5SH, 40 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (path /606FEFE1)
    (attr smd)
    (fp_text reference J4 (at 0 -3.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x40 (at 0 5.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 3.7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 13.05 -3) (end -13.05 -3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.05 4.9) (end 13.05 -3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -13.05 4.9) (end 13.05 4.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -13.05 -3) (end -13.05 4.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -9.75 -0.492893) (end -9.25 -1.2) (layer F.Fab) (width 0.1))
    (fp_line (start -10.25 -1.2) (end -9.75 -0.492893) (layer F.Fab) (width 0.1))
    (fp_line (start -10.16 -1.3) (end -10.16 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.65 4.5) (end 11.65 2.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.65 4.5) (end 11.65 4.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.65 2.76) (end -11.65 4.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.65 -1.3) (end 11.65 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 -1.3) (end 11.65 -1.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.65 -1.3) (end -11.65 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.16 -1.3) (end -11.65 -1.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.45 4.4) (end 0 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start 11.45 3.7) (end 11.45 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start 10.95 3.7) (end 11.45 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start 10.95 3.4) (end 10.95 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start 11.55 3.4) (end 10.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 11.55 -1.2) (end 11.55 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -1.2) (end 11.55 -1.2) (layer F.Fab) (width 0.1))
    (fp_line (start -11.45 4.4) (end 0 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start -11.45 3.7) (end -11.45 4.4) (layer F.Fab) (width 0.1))
    (fp_line (start -10.95 3.7) (end -11.45 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start -10.95 3.4) (end -10.95 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start -11.55 3.4) (end -10.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -11.55 -1.2) (end -11.55 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -1.2) (end -11.55 -1.2) (layer F.Fab) (width 0.1))
    (pad 40 smd rect (at 9.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 39 smd rect (at 9.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 38 smd rect (at 8.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 37 smd rect (at 8.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad4)"))
    (pad 36 smd rect (at 7.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad5)"))
    (pad 35 smd rect (at 7.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad6)"))
    (pad 34 smd rect (at 6.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad7)"))
    (pad 33 smd rect (at 6.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad8)"))
    (pad 32 smd rect (at 5.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J3-Pad9)"))
    (pad 31 smd rect (at 5.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J3-Pad10)"))
    (pad 30 smd rect (at 4.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad11)"))
    (pad 29 smd rect (at 4.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad12)"))
    (pad 28 smd rect (at 3.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad13)"))
    (pad 27 smd rect (at 3.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad14)"))
    (pad 26 smd rect (at 2.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-Pad15)"))
    (pad 25 smd rect (at 2.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad16)"))
    (pad 24 smd rect (at 1.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad17)"))
    (pad 23 smd rect (at 1.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad18)"))
    (pad 22 smd rect (at 0.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad19)"))
    (pad 21 smd rect (at 0.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad20)"))
    (pad 20 smd rect (at -0.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad21)"))
    (pad 19 smd rect (at -0.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad22)"))
    (pad 18 smd rect (at -1.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J3-Pad23)"))
    (pad 17 smd rect (at -1.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-Pad24)"))
    (pad 16 smd rect (at -2.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J3-Pad25)"))
    (pad 15 smd rect (at -2.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J3-Pad26)"))
    (pad 14 smd rect (at -3.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J3-Pad27)"))
    (pad 13 smd rect (at -3.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J3-Pad28)"))
    (pad 12 smd rect (at -4.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J3-Pad29)"))
    (pad 11 smd rect (at -4.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J3-Pad30)"))
    (pad 10 smd rect (at -5.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J3-Pad31)"))
    (pad 9 smd rect (at -5.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J3-Pad32)"))
    (pad 8 smd rect (at -6.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J3-Pad33)"))
    (pad 7 smd rect (at -6.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J3-Pad34)"))
    (pad 6 smd rect (at -7.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J3-Pad35)"))
    (pad 5 smd rect (at -7.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J3-Pad36)"))
    (pad 4 smd rect (at -8.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J3-Pad37)"))
    (pad 3 smd rect (at -8.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J3-Pad38)"))
    (pad 2 smd rect (at -9.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J3-Pad39)"))
    (pad 1 smd rect (at -9.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J3-Pad40)"))
    (pad MP smd rect (at -11.65 1.4) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at 11.65 1.4) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_arc (start 83.5 50.5) (end 85.5 50.5) (angle -180) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFF2))
  (gr_arc (start 83.5 40) (end 81.5 40) (angle -180) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFF1))
  (gr_line (start 81.5 35) (end 81.5 40) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFF0))
  (gr_arc (start 83.5 55.5) (end 81.5 55.5) (angle -180) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFEF))
  (gr_line (start 85.5 55.5) (end 85.5 50.5) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFEE))
  (gr_arc (start 83.5 35) (end 85.5 35) (angle -180) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFED))
  (gr_line (start 81.5 50.5) (end 81.5 55.5) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFEC))
  (gr_line (start 85.5 40) (end 85.5 35) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFEB))
  (gr_arc (start 34 55.5) (end 32 55.5) (angle -180) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFE6))
  (gr_line (start 32 50.5) (end 32 55.5) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFE5))
  (gr_arc (start 34 50.5) (end 36 50.5) (angle -180) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFE4))
  (gr_line (start 36 55.5) (end 36 50.5) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFE3))
  (gr_line (start 36 40) (end 36 35) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFE2))
  (gr_line (start 32 35) (end 32 40) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFE1))
  (gr_arc (start 34 40) (end 32 40) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 34 35) (end 36 35) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 30 30) (end 35 30) (layer Edge.Cuts) (width 0.05) (tstamp 6031FFE0))
  (gr_line (start 30 60) (end 30 30) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.5 60) (end 30 60) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.5 30) (end 87.5 60) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.5 30) (end 87.5 30) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 35 30) (end 82.5 30) (layer Edge.Cuts) (width 0.05))

  (segment (start 46.39 41.4) (end 46.39 42.65) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 46.39 42.65) (end 48.1 44.36) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 48.1 44.36) (end 48.1 51.3) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 48.1 51.3) (end 47.5 51.9) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 47.5 51.9) (end 45.65 51.9) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 45.39 41.4) (end 45.39 42.65) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 45.39 42.65) (end 46.15 43.41) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 46.15 43.41) (end 46.15 46.8736) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 46.15 46.8736) (end 47.425 48.1486) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 47.425 48.1486) (end 47.425 50.375) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 47.425 50.375) (end 46.9 50.9) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 46.9 50.9) (end 45.65 50.9) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 44.39 41.4) (end 44.39 43.1764) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 44.39 43.1764) (end 45.55 44.3364) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 45.55 44.3364) (end 45.55 47.9864) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 45.55 47.9864) (end 45.8136 48.25) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 45.8136 48.25) (end 46.8136 48.25) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 46.8136 48.25) (end 46.975 48.4114) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 46.975 48.4114) (end 46.975 49.825) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 46.975 49.825) (end 46.9 49.9) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 46.9 49.9) (end 45.65 49.9) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 43.39 41.4) (end 43.39 42.8128) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 43.39 42.8128) (end 45 44.4228) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 45 44.4228) (end 45 48.25) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 45 48.25) (end 45.65 48.9) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 74.625 50.025) (end 74.625 49.0497) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 74.625 49.0497) (end 74.65 49.0247) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 74.65 49.0247) (end 74.65 41.15) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 74.125 50.025) (end 74.125 49.0497) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 74.125 49.0497) (end 74.15 49.0247) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 74.15 49.0247) (end 74.15 41.15) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 73.625 50.025) (end 73.625 49.0497) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 73.625 49.0497) (end 73.65 49.0247) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 73.65 49.0247) (end 73.65 41.15) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 73.125 50.025) (end 73.125 49.0497) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 73.125 49.0497) (end 73.15 49.0247) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 73.15 49.0247) (end 73.15 41.15) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 72.625 50.025) (end 72.625 49.0497) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 72.625 49.0497) (end 72.65 49.0247) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 72.65 49.0247) (end 72.65 41.15) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 72.125 50.025) (end 72.125 49.0497) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 72.125 49.0497) (end 72.15 49.0247) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 72.15 49.0247) (end 72.15 41.15) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 71.625 50.025) (end 71.625 49.0497) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 71.625 49.0497) (end 71.65 49.0247) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 71.65 49.0247) (end 71.65 41.15) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 71.125 50.025) (end 71.125 49.0497) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 71.125 49.0497) (end 71.15 49.0247) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 71.15 49.0247) (end 71.15 41.15) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 70.625 50.025) (end 70.625 49.0497) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 70.625 49.0497) (end 70.65 49.0247) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 70.65 49.0247) (end 70.65 41.15) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 70.125 50.025) (end 70.125 49.0497) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 70.125 49.0497) (end 70.15 49.0247) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 70.15 49.0247) (end 70.15 41.15) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 69.625 50.025) (end 69.625 49.0497) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 69.625 49.0497) (end 69.65 49.0247) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 69.65 49.0247) (end 69.65 41.15) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 69.125 50.025) (end 69.125 49.0497) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 69.125 49.0497) (end 69.15 49.0247) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 69.15 49.0247) (end 69.15 41.15) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 68.625 50.025) (end 68.625 49.0497) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 68.625 49.0497) (end 68.65 49.0247) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 68.65 49.0247) (end 68.65 41.15) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 68.125 50.025) (end 68.125 49.0497) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 68.125 49.0497) (end 68.15 49.0247) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 68.15 49.0247) (end 68.15 41.15) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 67.625 50.025) (end 67.625 49.0497) (width 0.25) (layer F.Cu) (net 19))
  (segment (start 67.625 49.0497) (end 67.65 49.0247) (width 0.25) (layer F.Cu) (net 19))
  (segment (start 67.65 49.0247) (end 67.65 41.15) (width 0.25) (layer F.Cu) (net 19))
  (segment (start 67.125 50.025) (end 67.125 49.0497) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 67.125 49.0497) (end 67.15 49.0247) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 67.15 49.0247) (end 67.15 41.15) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 66.625 50.025) (end 66.625 49.0497) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 66.625 49.0497) (end 66.65 49.0247) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 66.65 49.0247) (end 66.65 41.15) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 66.125 50.025) (end 66.125 49.0497) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 66.125 49.0497) (end 66.15 49.0247) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 66.15 49.0247) (end 66.15 41.15) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 65.625 50.025) (end 65.625 49.0497) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 65.625 49.0497) (end 65.65 49.0247) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 65.65 49.0247) (end 65.65 41.15) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 65.125 50.025) (end 65.125 49.0497) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 65.125 49.0497) (end 65.15 49.0247) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 65.15 49.0247) (end 65.15 41.15) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 64.625 50.025) (end 64.625 49.0497) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 64.625 49.0497) (end 64.65 49.0247) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 64.65 49.0247) (end 64.65 41.15) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 64.125 50.025) (end 64.125 49.0497) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 64.125 49.0497) (end 64.15 49.0247) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 64.15 49.0247) (end 64.15 41.15) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 63.625 50.025) (end 63.625 49.0497) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 63.625 49.0497) (end 63.65 49.0247) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 63.65 49.0247) (end 63.65 41.15) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 63.125 50.025) (end 63.125 49.0497) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 63.125 49.0497) (end 63.15 49.0247) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 63.15 49.0247) (end 63.15 41.15) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 62.625 50.025) (end 62.625 49.0497) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 62.625 49.0497) (end 62.65 49.0247) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 62.65 49.0247) (end 62.65 41.15) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 62.125 50.025) (end 62.125 49.0497) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 62.125 49.0497) (end 62.15 49.0247) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 62.15 49.0247) (end 62.15 41.15) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 61.625 50.025) (end 61.625 49.0497) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 61.625 49.0497) (end 61.65 49.0247) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 61.65 49.0247) (end 61.65 41.15) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 61.125 50.025) (end 61.125 49.0497) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 61.125 49.0497) (end 61.15 49.0247) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 61.15 49.0247) (end 61.15 41.15) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 60.625 50.025) (end 60.625 49.0497) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 60.625 49.0497) (end 60.65 49.0247) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 60.65 49.0247) (end 60.65 41.15) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 60.125 50.025) (end 60.125 49.0497) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 60.125 49.0497) (end 60.15 49.0247) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 60.15 49.0247) (end 60.15 41.15) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 59.625 50.025) (end 59.625 49.0497) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 59.625 49.0497) (end 59.65 49.0247) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 59.65 49.0247) (end 59.65 41.15) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 59.125 50.025) (end 59.125 49.0497) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 59.125 49.0497) (end 59.15 49.0247) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 59.15 49.0247) (end 59.15 41.15) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 58.625 50.025) (end 58.625 49.0497) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 58.625 49.0497) (end 58.65 49.0247) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 58.65 49.0247) (end 58.65 41.15) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 58.125 50.025) (end 58.125 49.0497) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 58.125 49.0497) (end 58.15 49.0247) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 58.15 49.0247) (end 58.15 41.15) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 57.625 50.025) (end 57.625 49.0497) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 57.625 49.0497) (end 57.65 49.0247) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 57.65 49.0247) (end 57.65 41.15) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 57.125 50.025) (end 57.125 49.0497) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 57.125 49.0497) (end 57.15 49.0247) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 57.15 49.0247) (end 57.15 41.15) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 56.625 50.025) (end 56.625 49.0497) (width 0.25) (layer F.Cu) (net 41))
  (segment (start 56.625 49.0497) (end 56.65 49.0247) (width 0.25) (layer F.Cu) (net 41))
  (segment (start 56.65 49.0247) (end 56.65 41.15) (width 0.25) (layer F.Cu) (net 41))
  (segment (start 56.125 50.025) (end 56.125 49.0497) (width 0.25) (layer F.Cu) (net 42))
  (segment (start 56.125 49.0497) (end 56.15 49.0247) (width 0.25) (layer F.Cu) (net 42))
  (segment (start 56.15 49.0247) (end 56.15 41.15) (width 0.25) (layer F.Cu) (net 42))
  (segment (start 55.625 50.025) (end 55.625 49.0497) (width 0.25) (layer F.Cu) (net 43))
  (segment (start 55.625 49.0497) (end 55.65 49.0247) (width 0.25) (layer F.Cu) (net 43))
  (segment (start 55.65 49.0247) (end 55.65 41.15) (width 0.25) (layer F.Cu) (net 43))
  (segment (start 55.15 41.15) (end 55.15 42.1253) (width 0.25) (layer F.Cu) (net 44))
  (segment (start 55.125 50.025) (end 55.125 42.1503) (width 0.25) (layer F.Cu) (net 44))
  (segment (start 55.125 42.1503) (end 55.15 42.1253) (width 0.25) (layer F.Cu) (net 44))

)
