## KiBoM PCB Bill of Materials

Source File | E:\Users\Benjamin\Documents\tubcloud\Projekte\Waveshare_LCD_HAT\rgb_lcd_hat\rgb_lcd_pihat.sch
BoM Date | 21.02.2021 15:11:27
Schematic Version |
Schematic Date |
KiCad Version | Eeschema (5.1.4)-1
Component Groups | 34
Component Count (per PCB) | 48
Fitted Components (per PCB) | 48
Number of PCBs | 1
Total Component Count (for 1 PCBs) | 48

## Component Groups

Kicad Fields (default)

Generated Fields

User Fields

Empty Fields

| Description | Part | References | Value | Footprint | Quantity Per PCB | Datasheet | LCSC | Other Source
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | Unpolarized capacitor, small symbol | C_Small | C6 C7 C9 C11 | 100n | C_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 4 |  |  |
2 | Unpolarized capacitor, small symbol | C_Small | C3 | 10n | C_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 1 |  |  |
3 | Unpolarized capacitor, small symbol | C_Small | C8 | 220n | C_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 1 |  |  |
4 | Unpolarized capacitor, small symbol | C_Small | C1 C2 | 22p | C_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 2 |  |  |
5 |  | C_Polarized_Small-Device | C4 C5 C10 | 22u | CP_Elec_4x5.3 | 3 |  | C305355 |
6 | Schottky diode, small symbol | D_Schottky_Small | D3 | D_Schottky_Small | D_SMC | 1 |  | C353177 |
7 | Light emitting diode | LED | D1 | LED | LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 1 |  |  |
8 | Light emitting diode | LED | D2 | PWRLED | LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 1 |  |  |
9 | Mounting Hole without connection | MountingHole | H1 H2 H3 H4 | MountingHole | MountingHole_3.2mm_M3 | 4 |  |  |
10 | Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/) | Conn_01x03 | J5 | Conn_01x03 | PinHeader_1x03_P2.54mm_Vertical | 1 |  | C262381 |
11 |  | Conn_01x40-conn | J4 | Conn_01x40 | Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal | 1 |  | C283157 |
12 | Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/) | Conn_02x20_Odd_Even | J2 | RPI40 | PinSocket_2x20_P2.54mm_Vertical | 1 |  |  |
13 | Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/) | Conn_01x04 | J3 | TOUCH | TE_84953-4_1x04-1MP_P1.0mm_Horizontal | 1 |  |  |
14 |  | USB_C_Receptacle_USB2.0-Connector | J1 | USB_C_Receptacle_USB2.0 | USB_C_Receptacle_Palconn_UTC16-G | 1 |  | C319148 |
15 | Jumper, 3-pole, pins 1+2 closed/bridged | Jumper_3_Bridged12 | JP1 JP2 | Jumper_3_Bridged12 | SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm | 2 |  |  |
16 | Inductor, small symbol | L_Small | L1 | 22u | L_6.3x6.3_H3 | 1 |  |  |
17 | Inductor, small symbol | L_Small | L2 | L_Small | L_6.3x6.3_H3 | 1 |  |  |
18 |  | Logo-Custom_logo | LOGO1 | Logo | BB | 1 |  |  |
19 |  | Logo-Custom_logo | LOGO2 | Logo | julian_logo_4mm | 1 |  |  |
20 | N-MOSFET transistor, gate/source/drain | Q_NMOS_GSD | Q1 | ATM7002KNSA | SOT-23_Handsoldering | 1 |  | C915711 | X
21 | Resistor, small symbol | R_Small | R3 | 0R | R_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 1 |  |  |
22 | Resistor, small symbol | R_Small | R5 R6 | 1 | R_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 2 |  | C163871 |
23 | Resistor, small symbol | R_Small | R8 R9 R10 | 100k | R_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 3 |  |  |
24 | Resistor, small symbol | R_Small | R2 R4 | 180 | R_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 2 |  |  |
25 | Resistor, small symbol | R_Small | R1 | 20k | R_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 1 |  |  |
26 | Resistor, small symbol | R_Small | R7 | 450k | R_0603_1608Metric_Pad1.05x0.95mm_HandSolder | 1 |  |  |
27 |  | R_Potentiometer-Device | RV1 | 10 | Potentiometer_Bourns_3214J_Horizontal | 1 |  | C124638 |
28 | Switch, single pole double throw | SW_SPDT | SW1 | SW_SPDT | SW_SPDT_PCM12 | 1 |  | C397350 |
29 | test point | TestPoint | TP1 | 3V3_DISPLAY | TestPoint_Keystone_5000-5004_Miniature | 1 |  | C238122 |
30 | test point | TestPoint | TP2 | BG_LEDS | TestPoint_Keystone_5000-5004_Miniature | 1 |  | C238122 |
31 |  | AR1100 | U1 | AR1100 | SSOP-20_5.3x7.2mm_P0.65mm | 1 | https://ww1.microchip.com/downloads/en/DeviceDoc/41606B.pdf | C219149 |
32 |  | ME3102 | U3 | ME3102 | SOT-23-5_HandSoldering | 1 |  | C83223 |
33 |  | PT4103 | U2 | PT4103 | SOT-23-6_Handsoldering | 1 |  | C19861 |
34 |  | Crystal_GND24-device | Y1 | Crystal_GND24 | Crystal_SMD_3225-4Pin_3.2x2.5mm | 1 |  | C709175 |