(export (version D)
  (design
    (source E:\Users\Benjamin\Documents\tubcloud\Projekte\Waveshare_LCD_HAT\rgb_lcd_hat\FPC_4_extender\FPC_4_extender.sch)
    (date "20.02.2021 19:50:37")
    (tool "Eeschema (5.1.4)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source FPC_4_extender.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Conn_01x04)
      (footprint Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60328FBF))
    (comp (ref J2)
      (value Conn_01x04)
      (footprint Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60329B47)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri "D:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib")))
  (nets
    (net (code 1) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4))
      (node (ref J2) (pin 1)))
    (net (code 2) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref J2) (pin 2)))
    (net (code 3) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref J2) (pin 3)))
    (net (code 4) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref J2) (pin 4)))))