(export (version D)
  (design
    (source E:\Users\Benjamin\Documents\tubcloud\Projekte\Waveshare_LCD_HAT\FPC_Extender\FPC_40_4_extender\FPC_40_4_extender.sch)
    (date "20.02.2021 18:11:57")
    (tool "Eeschema (5.1.4)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source FPC_40_4_extender.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Conn_01x04)
      (footprint Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606F93E2))
    (comp (ref J2)
      (value Conn_01x04)
      (footprint Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606FA278))
    (comp (ref J3)
      (value Conn_01x40)
      (footprint Connector_FFC-FPC:Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x40) (description "Generic connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606FBFA7))
    (comp (ref J4)
      (value Conn_01x40)
      (footprint Connector_FFC-FPC:Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x40) (description "Generic connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606FEFE1)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x40)
      (description "Generic connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x40))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri "D:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib")))
  (nets
    (net (code 1) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4))
      (node (ref J2) (pin 1)))
    (net (code 2) (name "Net-(J3-Pad36)")
      (node (ref J4) (pin 5))
      (node (ref J3) (pin 36)))
    (net (code 3) (name "Net-(J3-Pad35)")
      (node (ref J4) (pin 6))
      (node (ref J3) (pin 35)))
    (net (code 4) (name "Net-(J3-Pad34)")
      (node (ref J4) (pin 7))
      (node (ref J3) (pin 34)))
    (net (code 5) (name "Net-(J3-Pad33)")
      (node (ref J3) (pin 33))
      (node (ref J4) (pin 8)))
    (net (code 6) (name "Net-(J3-Pad32)")
      (node (ref J4) (pin 9))
      (node (ref J3) (pin 32)))
    (net (code 7) (name "Net-(J1-Pad1)")
      (node (ref J2) (pin 4))
      (node (ref J1) (pin 1)))
    (net (code 8) (name "Net-(J1-Pad2)")
      (node (ref J2) (pin 3))
      (node (ref J1) (pin 2)))
    (net (code 9) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref J2) (pin 2)))
    (net (code 10) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref J4) (pin 40)))
    (net (code 11) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2))
      (node (ref J4) (pin 39)))
    (net (code 12) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3))
      (node (ref J4) (pin 38)))
    (net (code 13) (name "Net-(J3-Pad4)")
      (node (ref J3) (pin 4))
      (node (ref J4) (pin 37)))
    (net (code 14) (name "Net-(J3-Pad5)")
      (node (ref J3) (pin 5))
      (node (ref J4) (pin 36)))
    (net (code 15) (name "Net-(J3-Pad6)")
      (node (ref J3) (pin 6))
      (node (ref J4) (pin 35)))
    (net (code 16) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7))
      (node (ref J4) (pin 34)))
    (net (code 17) (name "Net-(J3-Pad8)")
      (node (ref J4) (pin 33))
      (node (ref J3) (pin 8)))
    (net (code 18) (name "Net-(J3-Pad37)")
      (node (ref J4) (pin 4))
      (node (ref J3) (pin 37)))
    (net (code 19) (name "Net-(J3-Pad9)")
      (node (ref J3) (pin 9))
      (node (ref J4) (pin 32)))
    (net (code 20) (name "Net-(J3-Pad10)")
      (node (ref J4) (pin 31))
      (node (ref J3) (pin 10)))
    (net (code 21) (name "Net-(J3-Pad11)")
      (node (ref J4) (pin 30))
      (node (ref J3) (pin 11)))
    (net (code 22) (name "Net-(J3-Pad38)")
      (node (ref J3) (pin 38))
      (node (ref J4) (pin 3)))
    (net (code 23) (name "Net-(J3-Pad12)")
      (node (ref J3) (pin 12))
      (node (ref J4) (pin 29)))
    (net (code 24) (name "Net-(J3-Pad13)")
      (node (ref J3) (pin 13))
      (node (ref J4) (pin 28)))
    (net (code 25) (name "Net-(J3-Pad14)")
      (node (ref J3) (pin 14))
      (node (ref J4) (pin 27)))
    (net (code 26) (name "Net-(J3-Pad25)")
      (node (ref J4) (pin 16))
      (node (ref J3) (pin 25)))
    (net (code 27) (name "Net-(J3-Pad26)")
      (node (ref J4) (pin 15))
      (node (ref J3) (pin 26)))
    (net (code 28) (name "Net-(J3-Pad27)")
      (node (ref J3) (pin 27))
      (node (ref J4) (pin 14)))
    (net (code 29) (name "Net-(J3-Pad28)")
      (node (ref J3) (pin 28))
      (node (ref J4) (pin 13)))
    (net (code 30) (name "Net-(J3-Pad29)")
      (node (ref J3) (pin 29))
      (node (ref J4) (pin 12)))
    (net (code 31) (name "Net-(J3-Pad30)")
      (node (ref J4) (pin 11))
      (node (ref J3) (pin 30)))
    (net (code 32) (name "Net-(J3-Pad31)")
      (node (ref J4) (pin 10))
      (node (ref J3) (pin 31)))
    (net (code 33) (name "Net-(J3-Pad24)")
      (node (ref J4) (pin 17))
      (node (ref J3) (pin 24)))
    (net (code 34) (name "Net-(J3-Pad39)")
      (node (ref J3) (pin 39))
      (node (ref J4) (pin 2)))
    (net (code 35) (name "Net-(J3-Pad40)")
      (node (ref J3) (pin 40))
      (node (ref J4) (pin 1)))
    (net (code 36) (name "Net-(J3-Pad15)")
      (node (ref J4) (pin 26))
      (node (ref J3) (pin 15)))
    (net (code 37) (name "Net-(J3-Pad23)")
      (node (ref J3) (pin 23))
      (node (ref J4) (pin 18)))
    (net (code 38) (name "Net-(J3-Pad22)")
      (node (ref J4) (pin 19))
      (node (ref J3) (pin 22)))
    (net (code 39) (name "Net-(J3-Pad21)")
      (node (ref J4) (pin 20))
      (node (ref J3) (pin 21)))
    (net (code 40) (name "Net-(J3-Pad20)")
      (node (ref J4) (pin 21))
      (node (ref J3) (pin 20)))
    (net (code 41) (name "Net-(J3-Pad19)")
      (node (ref J4) (pin 22))
      (node (ref J3) (pin 19)))
    (net (code 42) (name "Net-(J3-Pad18)")
      (node (ref J4) (pin 23))
      (node (ref J3) (pin 18)))
    (net (code 43) (name "Net-(J3-Pad17)")
      (node (ref J3) (pin 17))
      (node (ref J4) (pin 24)))
    (net (code 44) (name "Net-(J3-Pad16)")
      (node (ref J4) (pin 25))
      (node (ref J3) (pin 16)))))