(export (version D)
  (design
    (source /home/thomas/repositories/weihnachtsbaumblink/loetworkshop_tannenbaum.sch)
    (date "Do 22 Sep 2016 17:35:51 CEST")
    (tool "Eeschema 4.0.4-stable")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Loetworkshop Tannenbaum Wechselblinker")
        (company "Breadboarder e.V.")
        (rev 2)
        (date 2016-03-03)
        (source loetworkshop_tannenbaum.sch)
        (comment (number 1) (value "KiCAD Portierung"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value NE555)
      (footprint Housings_DIP:DIP-8_W7.62mm_LongPads)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LM555N-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56603E56))
    (comp (ref R2)
      (value 330k)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56604196))
    (comp (ref R1)
      (value 330k)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566042A3))
    (comp (ref R3)
      (value 330)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56604384))
    (comp (ref R5)
      (value 330)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566043CC))
    (comp (ref R7)
      (value 330)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 5660440B))
    (comp (ref R4)
      (value 270)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56604439))
    (comp (ref R6)
      (value 270)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 5660446A))
    (comp (ref R8)
      (value 270)
      (footprint Resistors_ThroughHole:Resistor_Horizontal_RM10mm)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566044B8))
    (comp (ref C2)
      (value 4u7)
      (footprint Capacitors_ThroughHole:C_Radial_D5_L11_P2.5)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part CP1-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566044E6))
    (comp (ref C1)
      (value C)
      (footprint Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part C-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56604635))
    (comp (ref LED9)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566046F8))
    (comp (ref LED10)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56604BFF))
    (comp (ref LED11)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56604C82))
    (comp (ref LED12)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56604CF2))
    (comp (ref LED5)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56605302))
    (comp (ref LED6)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56605308))
    (comp (ref LED7)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 5660530E))
    (comp (ref LED8)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 56605314))
    (comp (ref LED1)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566053DB))
    (comp (ref LED2)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566053E1))
    (comp (ref LED3)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566053E7))
    (comp (ref LED4)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum))
      (sheetpath (names /) (tstamps /))
      (tstamp 566053ED))
    (comp (ref P1)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E3FF81))
    (comp (ref SW1)
      (value SWITCH_INV)
      (footprint Buttons_Switches_ThroughHole:SW_Micro_SPST)
      (libsource (lib device) (part SWITCH_INV))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E40E9F)))
  (libparts
    (libpart (lib loetworkshop_tannenbaum-rescue) (part C-RESCUE-loetworkshop_tannenbaum)
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C-RESCUE-loetworkshop_tannenbaum))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib loetworkshop_tannenbaum-rescue) (part CP1-RESCUE-loetworkshop_tannenbaum)
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1-RESCUE-loetworkshop_tannenbaum))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib loetworkshop_tannenbaum-rescue) (part LED-RESCUE-loetworkshop_tannenbaum)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED-RESCUE-loetworkshop_tannenbaum))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib loetworkshop_tannenbaum-rescue) (part LM555N-RESCUE-loetworkshop_tannenbaum)
      (fields
        (field (name Reference) U)
        (field (name Value) LM555N-RESCUE-loetworkshop_tannenbaum))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name TR) (type input))
        (pin (num 3) (name Q) (type output))
        (pin (num 4) (name R) (type input))
        (pin (num 5) (name CV) (type input))
        (pin (num 6) (name THR) (type input))
        (pin (num 7) (name DIS) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib loetworkshop_tannenbaum-rescue) (part R-RESCUE-loetworkshop_tannenbaum)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R-RESCUE-loetworkshop_tannenbaum))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SWITCH_INV)
      (description inverseur)
      (fields
        (field (name Reference) SW)
        (field (name Value) SWITCH_INV))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive)))))
  (libraries
    (library (logical loetworkshop_tannenbaum-rescue)
      (uri /home/thomas/repositories/weihnachtsbaumblink/loetworkshop_tannenbaum-rescue.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(LED7-Pad2)")
      (node (ref LED7) (pin 2))
      (node (ref LED8) (pin 1)))
    (net (code 2) (name "Net-(LED10-Pad2)")
      (node (ref LED10) (pin 2))
      (node (ref LED11) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref LED6) (pin 2))
      (node (ref LED7) (pin 1))
      (node (ref LED2) (pin 2))
      (node (ref LED3) (pin 1)))
    (net (code 3) (name "Net-(LED3-Pad2)")
      (node (ref LED4) (pin 1))
      (node (ref LED3) (pin 2)))
    (net (code 4) (name "Net-(LED11-Pad2)")
      (node (ref LED11) (pin 2))
      (node (ref LED12) (pin 1)))
    (net (code 5) (name "Net-(LED12-Pad2)")
      (node (ref R8) (pin 1))
      (node (ref LED12) (pin 2)))
    (net (code 6) (name "Net-(LED8-Pad2)")
      (node (ref R6) (pin 1))
      (node (ref LED8) (pin 2)))
    (net (code 7) (name "Net-(LED4-Pad2)")
      (node (ref LED4) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 8) (name "Net-(LED1-Pad2)")
      (node (ref LED2) (pin 1))
      (node (ref LED1) (pin 2)))
    (net (code 9) (name "Net-(R1-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 7))
      (node (ref R1) (pin 1)))
    (net (code 10) (name "Net-(LED5-Pad2)")
      (node (ref LED5) (pin 2))
      (node (ref LED6) (pin 1)))
    (net (code 11) (name +9V)
      (node (ref R7) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref U1) (pin 4))
      (node (ref R2) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref SW1) (pin 3)))
    (net (code 12) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 13) (name "Net-(P1-Pad2)")
      (node (ref P1) (pin 2))
      (node (ref SW1) (pin 2)))
    (net (code 14) (name "Net-(SW1-Pad1)")
      (node (ref SW1) (pin 1)))
    (net (code 15) (name "Net-(LED10-Pad1)")
      (node (ref LED10) (pin 1))
      (node (ref LED9) (pin 2)))
    (net (code 16) (name "Net-(LED9-Pad1)")
      (node (ref R7) (pin 2))
      (node (ref LED9) (pin 1)))
    (net (code 17) (name "Net-(LED5-Pad1)")
      (node (ref R5) (pin 2))
      (node (ref LED5) (pin 1)))
    (net (code 18) (name "Net-(LED1-Pad1)")
      (node (ref LED1) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 19) (name GND)
      (node (ref U1) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref C2) (pin 2)))
    (net (code 20) (name "Net-(C2-Pad1)")
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 6))
      (node (ref R1) (pin 2))
      (node (ref C2) (pin 1)))))