* /home/thomas/ownCloud/Verein/Projekte/Workshop Lötänfänger/Tannenbaumplatine/kicad/weihnachtsbaumblink/loetworkshop_tannenbaum.cir

* EESchema Netlist Version 1.1 (Spice format) creation date: Fr 04 Dez 2015 17:26:14 CET

* To exclude a component from the Spice Netlist add [Spice_Netlist_Enabled] user FIELD set to: N
* To reorder the component spice node sequence add [Spice_Node_Sequence] user FIELD and define sequence: 2,1,0

* Sheet Name: /
U1  GND Net-_C2-Pad1_ Net-_LED10-Pad2_ +9V ? Net-_C2-Pad1_ Net-_D1-Pad1_ +9V NE555		
P1  GND +9V CONN_2		
R2  Net-_D1-Pad1_ +9V 330k		
R1  Net-_D1-Pad1_ Net-_C2-Pad1_ 330k		
R3  +9V Net-_LED1-Pad1_ 330		
R5  +9V Net-_LED5-Pad1_ 330		
R7  +9V Net-_LED9-Pad1_ 330		
R4  Net-_LED4-Pad2_ GND 270		
R6  Net-_LED8-Pad2_ GND 270		
R8  Net-_LED12-Pad2_ GND 270		
C2  Net-_C2-Pad1_ GND 4u7		
C1  +9V GND C		
LED9  Net-_LED9-Pad1_ Net-_LED10-Pad1_ LED		
LED10  Net-_LED10-Pad1_ Net-_LED10-Pad2_ LED		
LED11  Net-_LED10-Pad2_ Net-_LED11-Pad2_ LED		
LED12  Net-_LED11-Pad2_ Net-_LED12-Pad2_ LED		
LED5  Net-_LED5-Pad1_ Net-_LED5-Pad2_ LED		
LED6  Net-_LED5-Pad2_ Net-_LED10-Pad2_ LED		
LED7  Net-_LED10-Pad2_ Net-_LED7-Pad2_ LED		
LED8  Net-_LED7-Pad2_ Net-_LED8-Pad2_ LED		
LED1  Net-_LED1-Pad1_ Net-_LED1-Pad2_ LED		
LED2  Net-_LED1-Pad2_ Net-_LED10-Pad2_ LED		
LED3  Net-_LED10-Pad2_ Net-_LED3-Pad2_ LED		
LED4  Net-_LED3-Pad2_ Net-_LED4-Pad2_ LED		
D1  Net-_D1-Pad1_ Net-_C2-Pad1_ 1N4148		

.end
